|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| O.O. | ***16-01989*** | | | MISO No | ***1-11225810*** | File No. | 240801 |
| **Abnormal Operating Condition:** | | 230 kV Line M33R (Riel – Transcona East - Ridgeway) | | | | | |
| **Effective Dates:** | | | 2016-09-13 from 0830 to 2016-09-16 at 1800 CST  (2016-09-13 from 0830 to 2016-09-16 at 1800 EST) | | | | |
| **Standing Guide Reference:** | | | MH-IESO Standing Guide - Generation Pattern 3 (Summer 301- 450 MW's) | | | | |

|  |  |
| --- | --- |
| **Description of Work:** | M33R – Commission Ridgeway 230 kV Breaker R4, Change M33R Relay Setttings. Inspect/repair Ridgeway M33R Line/Ground Disconnects, address hotspots on M33R MOD, investigate limit switch on D16B, top up R16 SF6. |





|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** | **Export**:  None.  **Import**: If RTCA indicates that the loss F3M will cause overloads on WT34, transfer from IESO may need to be curtailed. |

|  |  |
| --- | --- |
| **MISO North RC Notes:** | MH\_ONT\_E (Export) SOL = 225 MW  MH\_ONT\_W (Import) SOL = 225 MW |
|  |  |
| **Special Instructions:** | **TOI Extensions** - This TOI may be extended until 23:59, by performing the following steps.  a) Verify system conditions to confirm there are no additional tie line facilities outages, or new internal MH outages.  b) Review RTCA to confirm there are no new contingencies.  c) Contact MISO to confirm there are no new outages, if there are no new outages provide notice to MISO that MH is extending the TOI.  d) Extend the outage in COLA  e) Update TLAP outage table  f) Provide notice to affected balancing authorities |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | S. Brooks | **Date:** | 2016 09 06 |

Copies to:

SOSS, System Control Centre NSSS, System Control Centre

GSSS, System Control Centre GSO, System Control Centre

Operating Order Ontario IESO

MISO – St. Paul MHEB OASIS

File 240801