|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| O.O. | **17-01087** | | | MISO No | **1-12544690** | File No. | 240801 |
| **Abnormal Operating Condition:** | | 230 kV Line K21W (Whiteshell to Kenora) | | | | | |
| **Effective Dates:** | | | 2017-01-18 from 1000 to 2017-01-18 at 1400 CDT  (2017-01-18 from 1100 to 2017-01-18 at 1500 EST) | | | | |
| **Standing Guide Reference:** | | | MH-IESO Standing Guide | | | | |

|  |  |
| --- | --- |
| **Description of Work:** | Kenora working on Kenora TS - K21W terminal required out of service for P&C to test status and conditions for new SPS.  Open at 230 kV Whiteshell Station and 230 kV Kenora Station.  (230 kV Line K21W will be Out of Service) |





|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** | **Export**: none   **Import**: none |

|  |  |
| --- | --- |
| **MISO North RC Notes:** | MH\_ONT\_E (Export) SOL = 190 MW  MH\_ONT\_W (Import) SOL = 190 MW |
|  |  |
| **Special Instructions:** | **TOI Extensions** - This TOI may be extended until 23:59, by performing the following steps.  a) Verify system conditions to confirm there are no additional tie line facilities outages, or new internal MH outages.  b) Review RTCA to confirm there are no new contingencies.  c) Contact MISO to confirm there are no new outages, if there are no new outages provide notice to MISO that MH is extending the TOI.  d) Extend the outage in COLA  e) Update TLAP outage table  f) Provide notice to affected balancing authorities |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | J. Thompson | **Date:** | 2017 01 09 |

Copies to:

SOSS, System Control Centre NSSS, System Control Centre

GSSS, System Control Centre GSO, System Control Centre

Operating Order Ontario IESO

MISO – St. Paul MHEB OASIS

File 240801