|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| O.O. | **N/A** | MISO No. | **N/A** | File No. | 240801 |
| **Normal Operating Condition:** | Up to 500 MW of TRM on the MHEX\_N interface is reserved for the delivery of CRSG. The CRSG release is reviewed weekly and is normally released at midnight for the next seven days. Current Status: Release 500 MW of CRSG on MHEX\_N |
| **Effective Dates:** |  2016-01-01 to 2016-12-31 |
| **Standing Guide Reference:** | MHEX Standing Guide  |

|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** | A) Prior to releasing CRSG, Manitoba Hydro System Operators must ensure that sufficient generation reserves are available within the Manitoba Hydro System relative to the amount of CRSG to be released.  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | Scott Brooks | **Date:** | 2016 - 12 - 30 |

Copies to:

 SOSS, System Control Centre NSSS, System Control Centre

 GSSS, System Control Centre GSO, System Control Centre

 MISO – St. Paul