|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| O.O. | **18-07064-OO** | MISO No. | **1-18471526** | File No. | 240801 |
| **Name of Outage:** | 230 kV Line M33R (Ridgeway - Transcona East - Riel) |
| **Effective Dates:** |  2018-06-02 from 02:43 to 2018-06-03 at 17:00 CDT(2018-06-02 from 02:43 to 2018-06-03 at 17:00 EST) |
| **Standing Guide Reference:** | MH-IESO Standing Guide - Generation Pattern 5 (Summer 166- 301 MW's) |

|  |  |
| --- | --- |
| **System****Posturing** | None required |
| **Description****of Work:** | Line forced out |





|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** | Export:Import: |

|  |  |
| --- | --- |
| **Special Notes to MISO North RC** | MH\_ONT\_E (Export) Transfer Limit = 200 MWMH\_ONT\_W (Import) Transfer Limit = 200 MWMH\_ONT\_E (Export) Transfer Limit During Offloads = 127 MWMH\_ONT\_W (Import) Transfer Limit During Offloads = 122 MW |

|  |  |
| --- | --- |
| **Special Instructions:**  | **TOI Extensions** - This TOI may be extended until 23:59 by performing the following steps:1. 1. Verify system conditions to confirm there are no additional tie line facilities outages, or new internal MH outages.
2. 2. Review RTCA to confirm there are no new contingencies.
3. 3. Contact MISO to confirm there are no new outages, if there are no new outages provide notice to MISO that MH is extending the TOI.
4. 4. Extend the outage in COLA.
5. 5. Update TLAP outage table.

6. Provide notice to affected balancing authorities. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | C. Kabaluk | **Date:** | **2018 06 02** |

Copies to:

 SPSO, System Control Centre NSSS, System Control Centre

 GSSS, System Control Centre GNSO, System Control Centre

 Operating Order Ontario IESO

 MHEB OASIS MISO – St. Paul

 File 240801