Revised Voltage Schedule for Frontier Generating Facility

Effective July 25, 2013, the bus voltage at the point of interconnection for Frontier generating facilities interconnected to the Entergy Texas transmission system shall be maintained according to the following schedule:

Frontier Generating Facility

All Hours: 1.01 P.U. voltage

The Revised Voltage Schedule specified above is a target voltage to be maintained within a tolerance band. The tolerance band specified for this Revised Voltage Schedule is +4 kV / -3 kV.

This guideline should be utilized until further notice. Any change to this guideline or notice of suspension of this guideline shall be communicated via a posting on the Entergy OASIS ‘Special Notice Postings’ page.